AedesX Mosquito Population Control Programme – Field Service Routine Checklist

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| S/NO | Routine Task Description | Frequency  | Jan  | Feb | Mar | April  | May | June | July | Aug | Sept | Oct | Nov | Dec |
| 1 | Visual Inspection on AedesX Smart Gravitrap | Monthly |  |  |  |  |  |  |  |  |  |  |  |  |
| 2 | Press Reset Button to check the functionality of the AedesX Smart Gravitrap | Monthly |  |  |  |  |  |  |  |  |  |  |  |  |
| 3 | Remove any foreign objects in the attraction zone | Monthly |  |  |  |  |  |  |  |  |  |  |  |  |
| 4 | Refill the water if needed | Monthly |  |  |  |  |  |  |  |  |  |  |  |  |
| 5 | Replace new battery ( 4X AA alkaline ) | Quarterly |  |  |  |  |  |  |  |  |  |  |  |  |
| 6 | Cleaning of AedesX unit ( optional ) | Quarterly  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

 Tick the box when servicing is carried out periodically

  

 Monthly Routine Service Protocol Video Quarterly Routine Service Protocol Video